## 1.4.4

- esp_tinyusb: Added HighSpeed and Qualifier device descriptors in tinyusb configuration
- CDC-ACM: Removed MIN() definition if already defined
- MSC: Fixed EP size selecting in default configuration descriptor

## 1.4.3

- esp_tinyusb: Added ESP32P4 support (HS only)

## 1.4.2

- MSC: Fixed maximum files open
- Added uninstall function

## 1.4.0

- MSC: Fixed integer overflows
- CDC-ACM: Removed intermediate RX ringbuffer
- CDC-ACM: Increased default FIFO size to 512 bytes
- CDC-ACM: Fixed Virtual File System binding

## 1.3.0

- Added NCM extension

## 1.2.1 - 1.2.2

- Minor bugfixes

## 1.2.0

- Added MSC extension for accessing SPI Flash on memory card https://github.jsk.asia/espressif/idf-extra-components/commit/a8c00d7707ba4ceeb0970c023d702c7768dba3dc

## 1.1.0

- Added support for NCM, ECM/RNDIS, DFU and Bluetooth TinyUSB drivers https://github.jsk.asia/espressif/idf-extra-components/commit/79f35c9b047b583080f93a63310e2ee7d82ef17b

## 1.0.4

- Cleaned up string descriptors handling https://github.jsk.asia/espressif/idf-extra-components/commit/046cc4b02f524d5c7e3e56480a473cfe844dc3d6

## 1.0.2 - 1.0.3

- Minor bugfixes

## 1.0.1

- CDC-ACM: Return ESP_OK if there is nothing to flush https://github.jsk.asia/espressif/idf-extra-components/commit/388ff32eb09aa572d98c54cb355f1912ce42707c

## 1.0.0

- Initial version based on [esp-idf v4.4.3](https://github.jsk.asia/espressif/esp-idf/tree/v4.4.3/components/tinyusb)
